Take Off Brief

Airport Plane

|  |  |  |
| --- | --- | --- |
| \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_  Freqs: ATIS T G  Wx: ATIS AWOS  Wind:  Sky:  Temps:  Altimeter:  Remarks:  Active RW  DA:  RW TODA:  LAHSO DIST None  LDA:  50/70:  Vr:  Destination:  On Course Hdg:  Dep directions:  Init Alt: |  |  |
| Emergency Procedures:  Engine Failure on TO  On Runway, gear down  Cut Power, hard braking  On climb out, gear down  Cut Power, land on RW  On climb out, gear up  Accel to Vsse, return to land  Single Engine:  300 feet straight ahead, 30 deg L R  500 feet straight ahead, 45 deg L R  1000 feet Poss return to airport  Fuel selector off, Mixture off,  Mags off, Master Switch off  AVIATE, NAVIGATE, COMMUNICATE |  |  |
| Landing Brief  Airport:  Freqs:  ATIS T G  T  G  ATIS Info:  Wind:  Sky:  Temps:  Altimeter:  Active RW:  Remarks:  DA:  LDA:  LAHSO: None |  |  |