Take Off Brief

 Airport Plane

|  |  |  |
| --- | --- | --- |
|  \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Freqs: ATIS T GWx: ATIS AWOSWind:Sky:Temps:Altimeter:Remarks:Active RWDA:RW TODA:LAHSO DIST NoneLDA:50/70: Vr:Destination: On Course Hdg:Dep directions:Init Alt: |  |  |
| Emergency Procedures:Engine Failure on TO On Runway, gear down Cut Power, hard braking On climb out, gear down Cut Power, land on RWOn climb out, gear up Accel to Vsse, return to landSingle Engine: 300 feet straight ahead, 30 deg L R 500 feet straight ahead, 45 deg L R 1000 feet Poss return to airportFuel selector off, Mixture off, Mags off, Master Switch offAVIATE, NAVIGATE, COMMUNICATE |  |  |
| Landing BriefAirport:Freqs:ATIS T GTGATIS Info:Wind:Sky:Temps:Altimeter:Active RW:Remarks:DA:LDA: LAHSO: None |  |  |